Firmware FCO2 Update pure nature 1.0 - 25.10.2008

includes/changes:

Serial picture 

P0 - Pic every 10 Sec
P1 - Pic every minute
P5 - Pic every 5 minutes
P3 - Pic every 30 minutes
P6 - Pic every 60 minutes

First Picture will be recorded after 10 Sec each mode
We recommend the FCO² extreme Battery Pack or external power for above modes!



Driver installation FCO2 firmware update

1. Shut down your virus scanner. Install the file STKO2H 2.O. Ignore certification warnings from MicroSoft (specially Vista)

2. Restart your computer.

3. Keep Cam "OFF" during installation process.

4. Press "Mode Button" at your FCO2 while connecting via USB-Cable to your Computer. 	

5. Start the program STK02HU-Reinstall.
   Select:
   DRAM: 0X35 
   DRAM SIZE: 8M

6. After approx. 90 secs program gives feed back! Update sucessful!

7. Disconnect the FlyCamone and switch it off and on again! (not your PC!)

8. Additional points in the menue are available now.


Remove the program  due to "installing" the program again.

